
**The UDP Bandmap**

Aki Yoshida JA1NLX

## 1. 0 GENERAL

## 5.1 Config

Select the Config menu item.



New UBM\_6AB

There are a lots of options. You may choose whatever you prefer now.

If you want to see highlight colors and tooltips information based on every mode then un-check "Highlight callsigns as "DIG" mode" This option works for displaying "QSOd B4" mark as well.

If you want to set the Logger32 frequency/mode from WSJT-X/JTDX then check ~~then check~~ “Allow WSJT/JTDX to set frequency/mode” Logger32 radio port must be closed. See paragraph 5.4 Start for related explanation and paragraph 5.0 Band Mode Selection Setup in the Logbook Entry ~~Emtry~~ topic.


If you want to see the Gridsquare then check "Show Gridsquares".

If you want to send SMS/eMail message then setup DX spot alerts (eMail/SMS/ScratchPad) in DX spot window, then check “Enable SMS/eMail message for new Country/Band/Mode”

Messages are sent once for each new Country/Band/Mode. if the Country is decoded again after 15 minutes, another message is sent. On the DX SPOT ALERT SETUP all checkboxes are ignored except the “CHECK THIS IF YOUR EMAIL ALERTS ARE BEING BLOCKED AS SPAM”

(See DX spot section in this Help)

Sample message below.



UBM\_6AB1

### Sub menu for Logging options



UBM\_6AC