**Data Terminal Window**

**Jim Hargrave W5IFP and Aki Yoshida JA1NLX**

**1.0 GENERAL**

The Data Terminal emulates a standard terminal program and provides the interface between Logger32 and Terminal Node Controllers.

It interfaces with generic standalone TNC2 and the multimode TNCs, such as KAM, PK-232, PK-900 and MFJ-1278. The program provides for mode changes with the click of the mouse. It does not support modems that depend on the software to provide the AX.25 packet protocol.

The Data Terminal also has a serial port, whose primary function is to control remote antenna switches. This port is interfaced with the Bands and Mode chart antenna selection. For setup details see “Setup Antenna selector” section in this help file.

Operation of the Data Terminal is accomplished in much the same fashion as the Sound Card Data window. Many of the same Macros are available to make communications easier for the user.

**2.0 SETUP**