New Macro

$hexbytes$               Data

Sends the hexadecimal string following the command to the Data Terminal, Antenna switch port.