

**The UDP Bandmap**

Aki Yoshida JA1NLX




UBM\_10A

Click "Highlight colors" to configure Gridsquare highlight colors and UDP Bandmap text color. If you prefer to see bold text for callsign who have called CQ then check "Show bold text who have called CQ"

.

new UBM\_11

Sample below.　The stations who are calling CQ now are displayed in Green text, the stations who have called CQ are displayed in Black/bold text and the stations who are working other stations are displayed in Black text.



new UBM\_11A

## 5.2. Clear

This clears UDP Bandmap.

## 5.3. Me

This opens the Calling Me UDP Bandmap and hide this item in the menu bar. See details in paragraph [Operation(4)](#8.0._OPERATION(4)).

## 5.4. Start

You should add items with a caption and shortcut.You may add another shortcut using unique radio name. See details in WSJT-X/JTDX Help.

If you start WSJT/JTDX from Start menu, the Logger32 radio serial port is closed before the digital application starts. WSJT-X/JTDX caption is replaced by shortcut caption + “& Logger32”and “X”is hidden in the title bar.



UBM\_11AB