**Digital Voice Keyer (DVK)**

# Geoff Anderson G3NPA

## 1.0 GENERAL

### 2.5 Shortcut Keys

The DVK supports the following hotkeys if the focus is on the DVK window:

* + <**F1**> to <**F8**>  Selects one of the Sound play buttons
  + <**Ctrl+L**> Turns Loop on
  + <**Ctrl+S**> Stops Play
  + <**Ctrl+A**> or <**Esc**> Aborts play.

If the focus is in the Logbook Entry Window ~~Log input window~~, then only the <**F1**> to <**F4**> and <Esc> keys will function.

**Note**: Intercept of the keys from the [Logbook Entry window](#_topic_LogbookEntryWindow) is by the [CW Machine](#_topic_CWMachineWindow), else the [Sound Card Data window](#_topic_SoundCardDataWindow1), else the DVK. If the CW Machine is loaded it will intercept the <**Fn**> keys. If the Sound Card Data window is loaded, it gets the keys. If neither of these is loaded, then the DVK gets the keys.